;
; AMI - The Asterisk Manager Interface
; 
; Third party application call management support and PBX event supervision
;
; This configuration file is read every time someone logs in
;
; Use the "show manager commands" at the CLI to list available manager commands
; and their authorization levels.
;
; "show manager command <command>" will show a help text.
;
; ---------------------------- SECURITY NOTE -------------------------------
; Note that you should not enable the AMI on a public IP address. If needed,
; block this TCP port with iptables (or another FW software) and reach it
; with IPsec, SSH, or SSL vpn tunnel
;
[general]
enabled = no
port = 5038
bindaddr = 0.0.0.0
;displayconnects = yes

;[mark]
;secret = mysecret
;deny=0.0.0.0/0.0.0.0
;permit=209.16.236.73/255.255.255.0
;
; If the device connected via this user accepts input slowly,
; the timeout for writes to it can be increased to keep it
; from being disconnected (value is in milliseconds)
;
; writetimeout = 100
;
; Authorization for various classes 
;read = system,call,log,verbose,command,agent,user
;write = system,call,log,verbose,command,agent,user
