;
; MGCP Configuration for Asterisk
;
[general]
;port = 2427
;bindaddr = 0.0.0.0

;[dlinkgw]
;host = 192.168.0.64
;context = default
;canreinvite = no
;line => aaln/2
;line => aaln/1

;; The MGCP channel supports the following service codes:
;; # - Transfer
;; *67 - Calling Number Delivery Blocking 
;; *70 - Cancel Call Waiting 
;; *72 - Call Forwarding Activation 
;; *73 - Call Forwarding Deactivation 
;; *78 - Do Not Disturb Activation 
;; *79 - Do Not Disturb Deactivation 
;; *8 - Call pick-up
;
; known to work with Swissvoice IP10s 
;[192.168.1.20] 
;context=local 
;host=192.168.1.20 
;callerid = "John Doe" <123> 
;callgroup=0      ; in the range from 0 to 63
;pickupgroup=0    ; in the range from 0 to 63
;nat=no 
;threewaycalling=yes 
;transfer=yes     ; transfer requires threewaycalling=yes. Use FLASH to transfer
;callwaiting=yes  ; this might be a cause of trouble for ip10s
;cancallforward=yes 
;line => aaln/1 
;

;[dph100]
;
; Supporting the DPH100M requires defining DLINK_BUGGY_FIRMWARE in
; chan_mgcp.c in addition to enabling the slowsequence mode due to
; bugs in the D-Link firmware
;
;context=local
;host=dynamic
;dtmfmode=none		; DTMF Mode can be 'none', 'rfc2833', or 'inband' or
				; 'hybrid' which starts in none and moves to inband.  Default is none.
;slowsequence=yes	; The DPH100M does not follow MGCP standards for sequencing
;line => aaln/1

; known to work with wave7optics FTTH LMGs
;[192.168.1.20]
;accountcode	= 1000		; record this in cdr as account identification for billing
;amaflags	= billing	; record this in cdr as flagged for 'billing', 'documentation', or 'omit'
;context	= local
;host		= 192.168.1.20
;wcardep	= aaln/*	; enables wildcard endpoint and sets it to 'aaln/*' another common format is '*'
;callerid 	= "Duane Cox" <123>	; now lets setup line 1 using per endpoint configuration...
;callwaiting	= no
;callreturn	= yes
;cancallforward = yes
;canreinvite	= no
;transfer	= no
;dtmfmode	= inband
;line => aaln/1			; now lets save this config to line1 aka aaln/1
;callerid 	= "Duane Cox" <456>	; now lets setup line 2
;callwaiting	= no
;callreturn	= yes
;cancallforward = yes
;canreinvite	= no
;transfer	= no
;dtmfmode	= inband
;line => aaln/2			; now lets save this config to line2 aka aaln/2
