;
; Asterisk Built-in mini-HTTP server
;
;
; Note about Asterisk documentation:
;   If Asterisk was installed from a tarball, then the HTML documentation should
;   be installed in the static-http/docs directory which is
;   (/var/lib/asterisk/static-http/docs) on linux by default.  If the Asterisk
;   HTTP server is enabled in this file by setting the "enabled", "bindaddr",
;   and "bindport" options, then you should be able to view the documentation
;   remotely by browsing to:
;       http://<server_ip>:<bindport>/static/docs/index.html
;
[general]
;
; The name of the server, advertised in both the Server field in HTTP
; response message headers, as well as the <address /> element in certain HTTP
; response message bodies. If not furnished here, "Asterisk/{version}" will be
; used as a default value for the Server header field and the <address />
; element. Setting this property to a blank value will result in the omission
; of the Server header field from HTTP response message headers and the
; <address /> element from HTTP response message bodies.
;
servername=Asterisk
;
; Whether HTTP/HTTPS interface is enabled or not.  Default is no.
; This also affects manager/rawman/mxml access (see manager.conf)
;
;enabled=yes
;
; Address to bind to, both for HTTP and HTTPS. You MUST specify
; a bindaddr in order for the HTTP server to run. There is no
; default value.
;
bindaddr=127.0.0.1
;
; Port to bind to for HTTP sessions (default is 8088)
;
;bindport=8088
;
; Prefix allows you to specify a prefix for all requests
; to the server.  The default is blank.  If uncommented
; all requests must begin with /asterisk
;
;prefix=asterisk
;
; sessionlimit specifies the maximum number of httpsessions that will be
; allowed to exist at any given time. (default: 100)
;
;sessionlimit=100
;
; session_inactivity specifies the number of milliseconds to wait for
; more data over the HTTP connection before closing it.
;
; Default: 30000
;session_inactivity=30000
;
; session_keep_alive specifies the number of milliseconds to wait for
; the next HTTP request over a persistent connection.
;
; Set to 0 to disable persistent HTTP connections.
; Default: 15000
;session_keep_alive=15000
;
; Whether Asterisk should serve static content from static-http
; Default is no.
;
;enable_static=yes
;
; Whether Asterisk should serve a status page showing the running
; configuration of this built-in HTTP server.
; Default is yes.
;
;enable_status=no
;
; Redirect one URI to another.  This is how you would set a
; default page.
;   Syntax: redirect=<from here> <to there>
; For example, if you are using the Asterisk-gui,
; it is convenient to enable the following redirect:
;
;redirect = / /static/config/index.html
;
; HTTPS support. In addition to enabled=yes, you need to
; explicitly enable tls, define the port to use,
; and have a certificate somewhere.
;tlsenable=yes          ; enable tls - default no.
;tlsbindaddr=0.0.0.0:8089    ; address and port to bind to - default is bindaddr and port 8089.
;
;tlscertfile=</path/to/certificate.pem>  ; path to the certificate file (*.pem) only.
;tlsprivatekey=</path/to/private.pem>    ; path to private key file (*.pem) only.
; If no path is given for tlscertfile or tlsprivatekey, default is to look in current
; directory. If no tlsprivatekey is given, default is to search tlscertfile for private key.
;
; To produce a certificate you can e.g. use openssl. This places both the cert and
; private in same .pem file.
; openssl req -new -x509 -days 365 -nodes -out /tmp/foo.pem -keyout /tmp/foo.pem
;
; tlscipher=                             ; The list of allowed ciphers
;                                        ; if none are specified the following cipher
;                                        ; list will be used instead:
; ECDHE-RSA-AES128-GCM-SHA256:ECDHE-ECDSA-AES128-GCM-SHA256:ECDHE-RSA-AES256-GCM-SHA384:
; ECDHE-ECDSA-AES256-GCM-SHA384:DHE-RSA-AES128-GCM-SHA256:DHE-DSS-AES128-GCM-SHA256:
; kEDH+AESGCM:ECDHE-RSA-AES128-SHA256:ECDHE-ECDSA-AES128-SHA256:ECDHE-RSA-AES128-SHA:
; ECDHE-ECDSA-AES128-SHA:ECDHE-RSA-AES256-SHA384:ECDHE-ECDSA-AES256-SHA384:
; ECDHE-RSA-AES256-SHA:ECDHE-ECDSA-AES256-SHA:DHE-RSA-AES128-SHA256:DHE-RSA-AES128-SHA:
; DHE-DSS-AES128-SHA256:DHE-RSA-AES256-SHA256:DHE-DSS-AES256-SHA:DHE-RSA-AES256-SHA:
; AES128-GCM-SHA256:AES256-GCM-SHA384:AES128-SHA256:AES256-SHA256:AES128-SHA:AES256-SHA:
; AES:CAMELLIA:DES-CBC3-SHA:!aNULL:!eNULL:!EXPORT:!DES:!RC4:!MD5:!PSK:!aECDH:
; !EDH-DSS-DES-CBC3-SHA:!EDH-RSA-DES-CBC3-SHA:!KRB5-DES-CBC3-SHA
;
; tlsdisablev1=yes                ; Disable TLSv1 support - if not set this defaults to "yes"
; tlsdisablev11=yes               ; Disable TLSv1.1 support - if not set this defaults to "no"
; tlsdisablev12=yes               ; Disable TLSv1.2 support - if not set this defaults to "no"
;
; tlsservercipherorder=yes        ; Use the server preference order instead of the client order
;                                 ; Defaults to "yes"
;
; The post_mappings section maps URLs to real paths on the filesystem.  If a
; POST is done from within an authenticated manager session to one of the
; configured POST mappings, then any files in the POST will be placed in the
; configured directory.
;
;[post_mappings]
;
; NOTE: You need a valid HTTP AMI mansession_id cookie with the manager
; config permission to POST files.
;
; In this example, if the prefix option is set to "asterisk", then using the
; POST URL: /asterisk/uploads will put files in /var/lib/asterisk/uploads/.
;uploads = /var/lib/asterisk/uploads/
;
